{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["武威职业学院药学院基础化学实训室设备采购项目询价表"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"武威职业学院药学院基础化学实训室设备采购项目询价表","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"merged":[[0,0,0,7],[7,1,7,7],[8,0,9,1],[8,2,9,7],[10,0,12,1],[10,2,12,4],[10,5,14,7],[13,0,14,1],[13,2,14,4],[15,0,15,1],[15,2,15,7],[16,0,16,1],[16,2,16,7],[17,0,17,1],[17,2,17,7],[18,0,18,7]]}
["武威职业学院药学院基础化学实训室设备采购项目询价表"]
["序号","名称","单位","数量","规格","单价","合计","备注"]
[1,"蛋白质检测仪","台",1,"7英寸以上液晶触摸屏显示；主控芯片ARM Cortex-A7 RK3288/4核处理器；12旋转通道；仪器尺寸约42*31*14cm"]
[2,"数显恒温磁力搅拌器加热套","台",12,"加热功率：350W；容量：1000ml；控温范围：RT-380℃，数显控温；调速范围：0-2600转/分。"]
[3,"球棍模型套装","台",10,"塑料材质，包含294个球，339根连接键，带收纳箱。"]
[4,"电子天平","台",8,"最大称量1000g，重复性0.01g，线性误差0.02g；USB充电；准确度等级III级；支持RS232接口连接计算机、打印机等设备；具有水平调节脚，水平气泡；LCD液晶屏显示。"]
[5,"旋转蒸发仪","台",2,"手自一体升降；真空度399.9pa以下；蒸发能力21m/min以上；自动控温，数字显示；功率1000W。"]
["总计","  大写：                                                 ￥：                    元"]
["服务承诺",null,"保证质量，服务周到！如有不合适，随时调换！"]
[]
["供货商地址",{"$nulls":4},"供货商（盖章）"]
[]
[]
["报价人员签字"]
[]
["询价评审意见"]
["询价人员签字",null,"               "]
["监督人员签字"]
["注：本询价表一式一份。"]